Layers: 4

PCB Thickness: 0.8

Impedance: no JLC7628

Layer stackup: [Layer sequence，L1：AntennaN\_220821\_CopperTop.ger，L2：AntennaN\_220821\_CopperMid.ger，L3：AntennaN\_220821\_CopperMid2.ger，L4：AntennaN\_220821\_CopperBottom.ger]

PCB Color: Green

Silkscreen: White

Surface Finish: HASL(with lead)

Deburring/Edge rounding: No

Outer Copper Weight: 1

Inner Copper Weight: 0.5

Gold Fingers: No

Flying Probe Test: Fully Test

Castellated Holes: no

Remove Order Number: No

Min hole size/diameter: 0.2/0.45mm↑

4-Wire Kelvin Test: No

Material Type: FR4-Standard Tg 130-140C

Appearance Quality: IPC Class 2 Standard

Confirm Production file: No